Week/Date
Problems	1st Week	2nd Week	3rd Week	4th Week	5th Week	………	nth Week	
	/	/	/	/	/	/	/	
1. Presence of garbage that might collect water								
2. Stagnant water in containers								
3. Stagnant water on uneven floor								
4. Stagnant water in choked gullies, sand traps etc.								
5. Construction materials/ equipment collecting stagnant water								
6. Stagnant water in disused tyres								
7. Stagnant water in trays underneath refrigerators and air-conditioners								
8. Stagnant water in bamboo stumps								
9. Others								
10. Others								
Name of Inspector								
Signature								
Weekly Mosquito Inspection Program for Construction Sites

Remarks:
��	The management of construction sites may design their own inspection program to meet specific needs 
��	Inspection personnel should be assigned to carry out weekly inspection.  If mosquito or potential breeding places for mosquitoes were found, immediate and appropriate follow up actions should be taken, including:
�Y	Remove stagnant water
�Y	Dispose of garbage properly
�Y	Cover water containers properly, and keep empty containers upside down to avoid collecting water
�Y	Fill bamboo stumps and uneven ground filled with sand, mud or cement
�Y	Remove garbage from gullies to avoid choking
�Y	Wrap up disused tyres or punch the tyres with large holes
�Y	Cover construction materials that might collect water properly